|  |
| --- |
| | Width Opening | Basic Gate | What You Need | Placement | |
| |-----------------|------------|---------------|-----------| |
| | 29”–31½” | Included with Gate | No extensions | - | |
| | 31½”–34½” | 1 G5.5 Kit | Gate + 1 extension | One end | |
| | 34½”–37” | 2 G5.5 Kits | Gate + 2 extensions | One on each end | |
| | 37”–40” | 1 G12.5 | Gate + 3 extensions | 2 on one end; 1 on other end | |
| | 40”–42½” | 1 G12.5 + 1 G5.5 Kit | Gate + 4 extensions | 3 on one end; 1 on other end | |
| | 42½”–45” | 2 G12.5 | Gate + 5 extensions | 3 on one end; 2 on other end | |
| | 45”–47½” | 2 G12.5 + 1 G5.5 Kit | Gate + 6 extensions | 3 on each end | |
|  |
| \*\*Note:\*\* Extensions must be added as shown. |
|  |